1: How to update Bitstream\_enable / scaler enables in video mode

Because scaler\_reg\_0 and scaler\_reg\_36 is not synced by vsync, so it can not be updated on frame and should only be updated after current frame finish. So use **interrupt intr-44 (snr\_done) to update those two register if necessary.**