1. It's always recommended to add CDM circuits between core-phy.
2. For phy-pcs or pcs-core it depends on which power domain pcs share with:

If pcs share power supply with phy, CDM circuit between pcs and core is recommended, if pcs share power with core, then pcs-phy is recommended.